**TEMSA Toilet Dump Instructions**

1. **USE COMMON SENSE!**
2. Locate RV drain hose bucket (located in supply bay door).
3. Put on safety equipment; gloves & goggles found in bucket.
4. Connect black end of hose to bus by sliding it over the nipple on the bottom drain valve and twisting a quarter turn. Pull down on connector to make sure it’s attached firmly.
5. Insert gray end that has an elbow into the receptacle in the ground.
6. Pull lower lever to open the waste valve. You should hear the flow of the waste – now open the upper valve.
7. Wait until you no longer hear the flow.
8. Close both upper & lower waste valves on the bus.
9. Disconnect hose from bus by turning the fitting counter-clockwise a quarter turn then pull fitting loose.
10. **RINSE HOSE AND PUT IT BACK INTO BUCKET ALONG WITH THE SAFETY SUPPLIES!**
11. Fill toilet with 2 – 3 gallons of water (just enough to be able to flush it).
12. Make entry into DVR stating that you have used the kit so shop staff can restock the supplies.